{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["CH 13 BPA","CH 13 BPA (2)","CH 13 BPA (3)","CH 13 BPA (4)"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":8,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CH 13 BPA","index":0,"n_rows":11,"n_cols":53,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,0,10,0],[0,1,1,41],[2,1,2,41],[3,2,3,37],[3,38,3,41],[4,2,4,37],[4,38,4,41],[5,2,5,37],[5,38,5,41],[6,2,6,37],[6,38,6,41],[7,2,7,37],[7,38,7,41],[8,2,8,37],[8,38,8,41],[9,2,9,37],[9,38,9,41],[10,2,10,37],[10,38,10,41]]}
[null,"Hose Valves"]
[]
[]
[null,95,"Are hose caps and / or adapters in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"YES"]
[null,96,"Are threads in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NO"]
[null,97,"Are valve handles in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,98,"Are gaskets in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SEE NOTE"]
[null,99,"Are valves free from leaks?"]
[null,100,"Are valves free from obstructions?"]
[null,101,"Are restricting devices present if required?"]
[null,102,"Have Class I and III system hose valves been tested by opening and closing the valves?"]

{"sheet":"CH 13 BPA (2)","index":1,"n_rows":11,"n_cols":53,"rows_kept":11,"cut":false,"hidden":false,"merged":[[8,38,8,41],[9,2,9,37],[9,38,9,41],[0,0,10,0],[0,1,1,41],[2,1,2,41],[3,2,3,37],[3,38,3,41],[4,2,4,37],[4,38,4,41],[5,2,5,37],[5,38,5,41],[6,2,6,37],[10,2,10,37],[10,38,10,41],[6,38,6,41],[7,2,7,37],[7,38,7,41],[8,2,8,37]]}
[null,"Hose Valves"]
[]
[]
[null,95,"Are hose caps and / or adapters in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"YES",null,null,null,null,null,null,null,null,null,null,null,null,null,"YES"]
[null,96,"Are threads in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,"NO"]
[null,97,"Are valve handles in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NO",null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,98,"Are gaskets in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,"SEE NOTE"]
[null,99,"Are valves free from leaks?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,100,"Are valves free from obstructions?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,101,"Are restricting devices present if required?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,102,"Have Class I and III system hose valves been tested by opening and closing the valves?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]

{"sheet":"CH 13 BPA (3)","index":2,"n_rows":11,"n_cols":53,"rows_kept":11,"cut":false,"hidden":false,"merged":[[8,38,8,41],[9,2,9,37],[9,38,9,41],[0,0,10,0],[0,1,1,41],[2,1,2,41],[3,2,3,37],[3,38,3,41],[4,2,4,37],[4,38,4,41],[5,2,5,37],[5,38,5,41],[6,2,6,37],[10,2,10,37],[10,38,10,41],[6,38,6,41],[7,2,7,37],[7,38,7,41],[8,2,8,37]]}
[null,"Hose Valves"]
[]
[]
[null,95,"Are hose caps and / or adapters in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"YES",null,null,null,null,null,null,null,null,null,null,null,null,null,"YES"]
[null,96,"Are threads in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,"NO"]
[null,97,"Are valve handles in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NO",null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,98,"Are gaskets in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,"SEE NOTE"]
[null,99,"Are valves free from leaks?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,100,"Are valves free from obstructions?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,101,"Are restricting devices present if required?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,102,"Have Class I and III system hose valves been tested by opening and closing the valves?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]

{"sheet":"CH 13 BPA (4)","index":3,"n_rows":11,"n_cols":53,"rows_kept":11,"cut":false,"hidden":false,"merged":[[8,38,8,41],[9,2,9,37],[9,38,9,41],[0,0,10,0],[0,1,1,41],[2,1,2,41],[3,2,3,37],[3,38,3,41],[4,2,4,37],[4,38,4,41],[5,2,5,37],[5,38,5,41],[6,2,6,37],[10,2,10,37],[10,38,10,41],[6,38,6,41],[7,2,7,37],[7,38,7,41],[8,2,8,37]]}
[null,"Hose Valves"]
[]
[]
[null,95,"Are hose caps and / or adapters in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"YES",null,null,null,null,null,null,null,null,null,null,null,null,null,"YES"]
[null,96,"Are threads in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,"NO"]
[null,97,"Are valve handles in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"NO",null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,98,"Are gaskets in place and in good condition?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A",null,null,null,null,null,null,null,null,null,null,null,null,null,"SEE NOTE"]
[null,99,"Are valves free from leaks?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,100,"Are valves free from obstructions?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,101,"Are restricting devices present if required?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]
[null,102,"Have Class I and III system hose valves been tested by opening and closing the valves?",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"N/A"]